SCBC Factory Tool Instruction for online mode

1. Install
Turn on setup application
Example:
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Runtime install
If it’s your first time installing and PC missing .Net4.5 runtime, software will install .Net4.5 first.
It will take a few minutes.
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After install, it will create a shortcut on the desktop
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2. Login
If use online mode, you must input the correct account and password to enter the operate page.
The account and password will be provided after permission confirmed. (See 5.2)
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After login:
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3. Config
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1. Select the Com port of TV
2. Input the order name 
3. Click submit button 
Then you can see the operate page and some basic message of the order:
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4. Testing
Focus on the testbox of SN, and scan the barcode of PCB, then it will trigger the testing.
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And you will see the burning key selected automatic. 
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5. Special note
5.1 Network preparation
Make sure the PC used for production connecting Internet.
Enter the following website, if it working, means the network is ok:
https://cn.uc.qhmoka.com/scbc-server
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[bookmark: _GoBack]5.2 Add permission for PC
Provide the Mac addresses of PC to us; we will add the permission for each user side.

Example:
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