SCBC Factory Tool Instruction for online mode

1. Install
Turn on setup application
Example:
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Runtime install
If it’s your first time installing and PC missing .Net4.5 runtime, software will install .Net4.5 first.
It will take a few minutes.
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After install, it will create a shortcut on the desktop
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2. Login
If use online mode, you must input the correct account and password to enter the operate page.
The account and password will be provided after permission confirmed. (See 5.2)
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After login:
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3. Config
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1. Select the Com port of TV
2. Input the order name 
3. Click preload mode
4. Click submit button 






If it’s your first time submit the order, the tool will start the download process of the key DB file.
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Ignore this message and click ok.

Then click the submit again
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And you can see the operate page and some basic message of the order:
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5. Testing
Focus on the testbox of SN, and scan the barcode of PCB, then it will trigger the testing.
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And you will see the burning key selected automatic. 
[bookmark: _GoBack][image: ]

6. Special note
6.1 Network preparation
Make sure the PC used for production connecting Internet.
Enter the following website, if it working, means the network is ok:
https://cn.uc.qhmoka.com/scbc-server
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6.2 Add permission for PC
Provide the Mac addresses of PC to us; we will add the permission for each user side.

Example:
[image: ]
6.3 Factory must provide the SN list of order before production, MID server system will distribute the keys depend on SN list and create the DB file. Then the factory tool will parse the DB file and burn the key into mainboard according to SN input from scanner.
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